ambient heat engine

sealed fluid boiling temp 10oC
air temp 25oC


fluid boils
release charge into cylinder
cylinder expands to 120% of normal expansion
liquid condenses
pump liquid back into fluid resevoir

metal plates for fluid res for greater surface area
additional cooling of gas [metal plates]

surrounding air cools
air at power usage site heats
modest power output due to tempreture difference








