10-layer chip . TTL.



	north-south connections

	insulator

	east-west connections

	insulator

	positive rail

	resistor

	n

	p

	n

	neg rail





make the layers thicker to reduce capacitance and increase

maximum frequency


