large scale proc.



netw. instruction set


load progr into internal mem e.g. 1024 bytes

send to processor 1, 2, 3 or 4

data processed signal

receive from 1, 2, 3 or 4






		
		+---+---+...
		|   |   |
		+---+---+...
		|   |   |
		+---+---+...


                   ^
	           |		
		   |

		data in

