control thry.


sampled resetting


move from 12,000 to 15,000 feet



thrust, 0 to 10

linear feedback leads to oscillation




sampled


set thrust level

wait 10 seconds

set thrust level to new setting

wait 10 seconds

repeat until level is obtained

check sampling rate, stability etc.

