Starting large diesel engines

1. lqd. similar to explosive, combust time 1 sec, cylnder with
	pstn. at top
	
2. injectors with heating element, heat to 1000oC, larger
	quantties. than usual
	
3. until ht./norml spd.

