vhcl project, hot climates


cane mat sides, permanent canvas roof, no side windows

two seats at front, bench seat at back


1.4 Litre, 1 cylinder engine


fuel efficiency very important


strengthened bicycle type wheels


top speed 55 kmh


starting by compressed air cylinder, recharged when driving, 

//	starting handle to compress air if not full

	small electric motor to recharge the air cylinder if necessary

	cylinder 2 ltr, 18 atm

	
2 gear speeds


clutch, chain drive gearbox, selectable chain set


lockable 2mx1mx0.5m cane storage, metal vertical latch, optional padlock
