sec.

facilities for wild locations



workshed

	30ft x 60ft x 18ft
	
	windows along each side, 3ft x 5.5ft in size, spaced 12ft apart



	wire mesh 1/4 inch diameter wire, 4 inches apart


	mesh section 

		18ft x 30ft x 16ft (made of wire mesh not solid tin panels)


		out from one side


		allows walking out to look at the surrounding area without being attacked



		see separate drawing (sec workshed)
		



house

	normal house


	fence 58ft from the house

	metal poles, 1inch in diameter, 5 inches apart, 11ft high, metal spikes on top (not sharp)





	


	